;$Revision:   1.137  $
Chips and Technologies, Inc.
DR655xx Display Driver Package
Release Notes for Windows 95

                             DR655xx
                     Display Driver Package
                  Release Notes for Windows 95

Revision:   Preliminary Production Version 2.1.8
Release Date:  August 12, 1997
=================================================

1. Fixed palette not set problem when force from 16BPP to 8BPP.

2. Fixed a problem when free memory size on heap becomes zero.
	  
Revision:   Preliminary Production Version 2.1.7
Release Date:  August 11, 1997
=================================================
1. Fixed a hang problem with 1 MB of video memory in
   800x600x16 CRT mode on a DSTN panel. (Issue #537).

2. Fixed problem with garbage at the top of the screen when playing
   ActiveMovie nonoverlay, going to full screen DOS, making it windowed
   then changing between US and JP.

3. Fixed NTSC/PAL overlay alignment problems. (Issue #517).


Revision:   Preliminary Production Version 2.1.6
Release Date:  August 05, 1997
=================================================
1. Fixed Panel Status detection problem.


Revision:   Preliminary Production Version 2.1.5
Release Date:  July 29, 1997
=================================================
1. This is a custom release.


Revision:   Preliminary Production Version 2.1.4
Release Date:  July 29, 1997
=================================================
 1.Fixed dynamic display change during ActiveMovie
   is switched back to previous display when ActiveMovie
   terminates. (Issue #443).

 2.Fixed NTSC/PAL problem.


Revision:   Preliminary Production Version 2.1.3
Release Date:  July 25, 1997
=================================================
1. Added TV Attributes button on CHIPSDSP property page
   The button only enabled when display in TV mode

2. TV attributes Dialog, can switch from pannig to non-
   panning, Filtering on and off, interlaced and non-
   interlaced.  Also, CHIPS button fix in Japanese Win 95.

3. Fixed POPUP corruption problem. Added POPUP
   memory adjustment. (Issue #494).

4. Fixed MS Access garbage problem when scroll records (90 degree).

5. Fixed Panel Status detection problem.

6. Fixed NTSC DOS problem.


Revision:   Preliminary Production Version 2.1.1
Release Date:  July 18, 1997
=================================================
1. Fixed overlay panning problem. (Issue #486).

2. Fixed virtual desktop overlay vertical alignment problem. (Issue #485).


Revision:   Preliminary Production Version 2.1.0
Release Date:  July 17, 1997
=================================================
1. This is a custom release.


Revision:   Preliminary Production Version 2.0.9
Release Date:  July 17, 1997
=================================================
1. Fixed a screen corruption problem with Japanese Win 95 when playing
   overlay then go to full screen DOS and making it a windowed DOS.

2. Added generic mode support.

3. Fixed stretched text problem in Korean Win 95 full screen DOS.

4. Fixed virtual desktop overlay alignment problem. (Issue #485).

5. Fixed overlay panning problems. (Issue #486).

6. CHIPSVPM.DLL is version 1.1.0.113.


Revision:   Preliminary Production Version 2.0.8
Release Date:  June 27, 1997
=================================================
1. Fixed problem with allowing stretching instantaneously. (Issue #460).

2. Fixed 65555 NTSC TV out alignment problem. (Issue #364).

3. Use VGA BIOS low resolution modes if available.


Revision:   Preliminary Production Version 2.0.7
Release Date:  June 23, 1997
=================================================
1. Fixed screen corruption after starting Monster Truck Madness in
   1280x1024x8 then exiting.

2. Fixed butterfly overlay wrong key color problem.

3. Allow maximum width in CHIPSVPM to be 1024.

4. Fixed noise problem with ChipsTV.  CHIPSVPM.DLL is version 1.1.0.112.

5. Updated CHIPSMM.INI for TFT 800x600 panel 50MHz dot clock on a 65554
   with 40MHz memory clock.


Revision:   Preliminary Production Version 2.0.6
Release Date:  June 19, 1997
=================================================
1. Added 16 bit and 24 bit support for custom driver.

2. Solved problem with performance in 65555 because the software cursor
   was accidentally enabled all the time. (Issue #465).

3. Fixed problem where the color key was not enabled for overlay.

4. This is a custom release.


Revision:   Preliminary Production Version 2.0.5
Release Date:  June 16, 1997
=================================================
1. Fixed WinBench 95 GWM9 hang problem.

2. Fixed MPEG wrap problem when source pitch is greater than 352.
   (Issue #403).


Revision:   Preliminary Production Version 2.0.4
Release Date:  June 10, 1997
=================================================
1. Added VPM display switch stretched graphic mode support.

2. Fixed custom driver problem with moving windows around
   and display corruption on background and in window. (Issue #428).

3. Fixed custom driver problem with mouse corrupt when vertical
   line replication is enabled. (Issue #429).

4. Fixed custom driver problem with cursor position showing garbage
   in MS Paint. (Issue #435).

5. Fixed problem with losing overlay after going to full screen DOS
   and exiting.

6. Fixed problem with random hanging when exiting full screen DOS on
   Japanese Win 95. (Issue #445).

7. CHIPSVPM.DLL is version 1.1.0.111.

8. This is a custom release.


Revision:   Preliminary Production Version 2.0.3
Release Date:  June 3, 1997
=================================================
1. Fixed booting problem with 4 bpp modes.

2. Fixed general protection fault with TranXit in Japanese Win 95.
   (Issue #439).


Revision:   Preliminary Production Version 2.0.2
Release Date:  May 29, 1997
=================================================
1. Fixed MS word string broken problem.


Revision:   Preliminary Production Version 2.0.1
Release Date:  May 29, 1997
=================================================
1. Fixed Japanese Win95 font cache hang problem. (Issue #424).

2. Fixed MPEG playback wrap problem when source pitch is greater
   than 352. (Issue #403).

3. This is a custom release.


Revision:   Preliminary Production Version 1.5.9
Release Date:  May 21, 1997
=================================================
1. Fixed MS Word text string corrupt problem. (Issue #360, #371, #416).

2. CHIPSDSP added a stretch screen feature. The feature
   is hidden by default.


Revision:   Preliminary Production Version 1.5.8
Release Date:  May 19, 1997
=================================================
1. Fixed font cache location problem.

2. Fixed MS Outlook text string corrupt problem.

3. Added VPM support for graphics stretch overlay. (Issue #387).

4. Fixed interlaced odd line problem during video playback. (Issue #388).

5. Removed 240 line limit in CHIPSVPM.DLL. (Issue #386, #404).

6. CHIPSVPM.DLL is version 1.1.0.110.


Revision:   Preliminary Production Version 1.5.7
Release Date:  May 09, 1997
=================================================
1. Fixed problem in modes that do not have memory for virtual mode 12.
   If play overlay and open a windowed DOS box the cursor may become
   garbage.

2. CHIPSVPM.DLL is version 1.1.0.108.


Revision:   Preliminary Production Version 2.0.0
Release Date:  May 09, 1997
=================================================
1. Fixed no overlay problem when have 1 MB video memory for 640x480
   and 800x600 modes.

2. CHIPSVPM.DLL is version 1.1.0.109.

3. This is a custom release.


Revision:   Preliminary Production Version 1.5.6
Release Date:  April 30, 1997
=================================================
1. Fixed corruption with Flying Windows screen saver. (Issue #382).

2. Fixed overlay problem in stretched mode. (Issue #387).


Revision:   Preliminary Production Version 1.5.5
Release Date:  April 29, 1997
=================================================
1. Fixed a problem with overlay playback when switch CR/SM/FP.

2. Fixed a problem with CHIPSDSP.DLL displaying the wrong text
   for custom mode 1024x600x8 and 1024x600x16.

3. Fixed a problem with CHIPSDSP.DLL on Japanese Win 95.


Revision:   Preliminary Production Version 1.5.4
Release Date:  April 23, 1997
=================================================
1. Modified CRT modes 320x240, 400x300 and 512x384 to run at a lower
   refresh rate.

2. Fixed a problem with corrupt font after running VMTEST.

3. Fixed a problem with flashing when switch from ActiveMovie
   full screen to windowed.

4. Eliminated a 24 bpp custom DirectDraw mode.


Revision:   Preliminary Production Version 1.5.3
Release Date:  April 17, 1997
=================================================
1. Fixed a problem with 4 bpp modes when we have virtual desktops.

2. Fixed a boot problem with modes 1024x768x256 in a 1 MB system
   and 1280x1024x24 in a 4 MB system.

3. Fixed Japanese help (DBCS) in CHIPSDSP.DLL.

4. Fixed a problem with CHIPSVPM.DLL with right side wrap and always
   set to field mode capture.  This is version 1.1.0.108.


Revision:   Preliminary Production Version 1.5.2
Release Date:  April 14, 1997
=================================================
1. Enable 1024x600x8 and 1024x600x16.  Will be available if VGA BIOS
   supports it.

2. Uncommented United Kingdom in CHIPSDSP.INI.


Revision:   Preliminary Production Version 1.5.1
Release Date:  April 11, 1997
=================================================
1. Fixed a screen corruption problem with Media Player and Japanese
   DOS window.

2. Fixed a problem with changing resolutions.


Revision:   Preliminary Production Version 1.5.0
Release Date:  April 09, 1997
=================================================
1. Fixed a screen corruption problem with Media Player and DOS window.

2. Fixed problem with a dead overlay on the screen when do a dynamic
   mode change.

3. Fixed problem with a dead overlay on the screen when the 3D Maze
   screen saver comes up.

4. Fixed problem with a dead overlay on the screen when go out to
   full screen DOS and come back.


Revision:   Preliminary Production Version 1.4.9
Release Date:  April 04, 1997
=================================================
1. Fixed a boot problem with 1 MB of video memory in
   800x600x16 CRT mode.

2. Fixed a problem in CHIPSVPM.DLL so when we have playback
   with a ZV port we can see more of the picture.
   This is version 1.1.0.107.

3. Fixed problem with doing a "dir b:" in a DOS box.

4. Fixed a problem with corrupt icons after going to 3D Maze screen
   saver then low-power standby.


Revision:   Preliminary Production Version 1.4.8
Release Date:  March 31, 1997
=================================================
1. Fixed the return value in DestroySurface that the driver did
   not handle it so DirectDraw can handle freeing memory.


Revision:   Preliminary Production Version 1.4.7
Release Date:  March 31, 1997
=================================================
1. Fixed a panning problem with WHQL Overfly when the butterfly
   is near the top of the screen.

2. Fixed the return value in DestroySurface that the driver handled it.

3. Enabled HW specific features for 65555/68554; it also
   has HW panning enabled.  These will be enabled from now on.


Revision:   Preliminary Production Version 1.4.6
Release Date:  March 27, 1997
=================================================
1. Fixed problem where DirectDraw custom modes for 1024x600
   were not enabled.

2. This is a custom release for 1024x600 panel and modes.


Revision:   Preliminary Production Version 1.4.5
Release Date:  March 25, 1997
=================================================
1. Fixed the problem when using control panel to change display mode
from BOTH to LCD.  The machine hanged and the screen became blank.


Revision:   Preliminary Production Version 1.4.4
Release Date:  March 21, 1997
=================================================
1. Fixed problem where vertical interpolation was not being enabled.


Revision:   Preliminary Production Version 1.4.3
Release Date:  March 19, 1997
=================================================
1. Enabled HW specific features for 65555/68554; it also has HW 
   panning enabled.  These are for this release only.


Revision:   Preliminary Production Version 1.4.2
Release Date:  March 19, 1997
=================================================
1. During installation will also copy over CHIPSDSP.INI and
   JAPANESE.HLP. In CHIPSDSP.INI we added language support.  We
   can detect what language the system is using and bring up
   the right text in the control panel property page. The language
   caption is set in CHIPSDSP.INI file.

2. This is a custom release for 1024x600 panel and modes.


Revision:   Preliminary Production Version 1.4.1
Release Date:  March 14, 1997
=================================================
1. Added custom mode resolutions 1024x600 to DirectDraw but
   they are only enabled for custom driver.

2. Modifed the 320x200 resolutions to run at a lower refresh rate.


Revision:   Preliminary Production Version 1.4.0
Release Date:  March 10, 1997
=================================================
1. Enabled HW specific features for 65555.  This is for this release only.


Revision:   Preliminary Production Version 1.3.9
Release Date:  March 10, 1997
=================================================
1. Fixed video overlay alignment problem in all NTSC/PAL interlaced modes.

2. Fixed video overlay alignment problem in custom mode 1024x600
   for interlaced and 60 Hz refresh.

3. Fixed Overfly having a green background when using YUY2.


Revision:   Preliminary Production Version 1.3.8
Release Date:  March 04, 1997
=================================================
1. Changed CHIPSVPM.DLL to fix some stray black lines on left
   edge of capture window.  This is version 1.1.0.106.


Revision:   Preliminary Production Version 1.3.7
Release Date:  February 21, 1997
=================================================
1. Changed custom mode 1024x600x24 to require 2 MB instead of
   3 MB of memory.
2. This is a custom release for 1024x600 panel and modes.


Revision:   Preliminary Production Version 1.3.6
Release Date:  February 18, 1997
=================================================
1. Same release of Version 1.3.5 with custom features removed.


Revision:   Preliminary Production Version 1.3.5
Release Date:  February 18, 1997
=================================================
1. Added custom mode 1024x600x4.

2. New CHIPSVPM.DLL.  This is version 1.1.0.105.

3. New CHIPSDSP.DLL.

4. Custom release for 1024x600 panel and modes.


Revision:   Preliminary Production Version 1.3.4
Release Date:  February 14, 1997
=================================================
1. Fixed mouse problems (area beneath it) in 16 color modes.


Revision:   Preliminary Production Version 1.3.3
Release Date:  February 10, 1997
=================================================
1. Eliminated CHTDD16.DLL.

2. Added low resolution modes for DirectX games.


Revision:   Preliminary Production Version 1.3.2
Release Date:  February 04, 1997
=================================================
1. Fixed problem with allowing multiple overlay surfaces
   in ActiveMovie when we can only allow one.


Revision:   Preliminary Production Version 1.3.1
Release Date:  January 28, 1997
=================================================
1. Fixed video overlay alignment problem in NTSC 640x480 and
   PAL 800x600 interlaced modes.


Revision:   Preliminary Production Version 1.3.0
Release Date:  January 22, 1997
=================================================
1. Has offscreen bitmap support.


Revision:   Preliminary Production Version 1.2.9
Release Date:  January 20, 1997
=================================================
1. Fixed SetColorKey problem.

2. Fixed problem if a requested resolution is not supported.

3. Added support for external frame buffer in DSTN panel types.


Revision:   Preliminary Production Version 1.2.8
Release Date:  January 13, 1997
=================================================
1. Enable ellipse and polygon in driver.


Revision:   Preliminary Production Version 1.2.7
Release Date:  January 08, 1997
=================================================
1. Fixed Tddraw Test Case 35 when doing source transparent blts in
   the right to left direction.

2. Fixed problem with not waiting for vertical blank time to do a flip
   in DirectDraw.

3. Implemented DirectDraw SetColorKey.


Revision:   Preliminary Production Version 1.2.6
Release Date:  December 19, 1996
=================================================
1. Fixed Control panel CHIPSDSP <Up> and <Down> Key of
   "Monitor Type" selection problem.

2. Fixed a problem on VL bus machine that when open windowed DOS 
   first time after restarted Windows, it takes several seconds.
   This also fixed problems that some VGA modes didn't work in 
   windowed DOS.


Revision:   Preliminary Production Version 1.2.5
Release Date:  December 4, 1996
=================================================
1. Fixed OSR2 ActiveMovie not using hardware overlay problem.


Revision:   Preliminary Production Version 1.2.4
Release Date:  November 8, 1996
=================================================
1. Same as version 1.2.3 but compiled with offscreen bitmap.


Revision:   Preliminary Production Version 1.2.3
Release Date:  November 8, 1996
=================================================
1. Performance fix for CorelDraw.

2. Initialize overlay values for DirectDraw in capabilities
   structure.

3. Fixed problems with WHQL Overfly when overlay same as primary surface.


Revision:   Preliminary Production Version 1.2.2
Release Date:  November 5, 1996
=================================================
1. Fixed screen saver shut down power and offscreen bitmap get lost
problem.

2. Fixed WHQL Overfly panning problem.

3. Removed fix for the problem of the screen flashing twice
after resume because of an OSR2 problem.

4. Fixed problem that 256 color mode cannot be set correctly in full
screen DOS.

5. Fixed problem that mode 12 cannot be set correctly in full screen DOS.


Revision:   Preliminary Production Version 1.2.1
Release Date:  October 29, 1996
=================================================
1. Same as version 1.2.0 but compiled for no offscreen bitmap.


Revision:   Preliminary Production Version 1.2.0
Release Date:  October 29, 1996
=================================================

1. Fixed a wrong color (color translation) problem on all 256 color
   mode in LION KING application when CTRL_ESC is pressed on and then
   restored to LION KING windows again.

2. Updated CHIPSMM.INI in section Capture554x40 CRT_640x480x16x85
   CaptureInterpolX.

3. Fixed the problem of the screen flashing twice after resume.

4. Fixed the problem of garbage in CRT mode after resume.

5. Fixed problem with panning in NTSC when panning turned on mistakenly.

6. Fixed a screen corruption problem caused by moving cursor while 
   MYST is changing mode.

7. Fixed DOOM2 flashing problem.

8. Fixed MS Plus wallpaper problems.

9. Fixed a corruption problem when returning to un-supported Windows
mode on 65548.

10. Fixed problem with text mode font stretched in full screen DOS.


Revision:   Preliminary Production Version 1.1.8
Release Date:  October 3, 1996
=================================================

1.  Fixed a problem in Korean Windows that text is stretched after
    going to full screen DOS.

2.  Fixed a panning problem in 1024x768 mode on a 1024x600 panel.

3.  Fixed some typos in ModeInfo table.

4.  Fixed corruption problem when in a CRT only mode, go out to
    DOS box, change to simultaneous mode then exit.

5.  Fixed windowed FoxBear white background boxes appearing when
    Microsoft Office is opened.  This was for 65554.

6.  Updated Chipsmm.ini for 65554 40 MHz mclock TFT 640x480 and
    TFT 800x600 panel for all modes.  Updated also the maximum buffer
    width for 65554 40 MHz mclock for all CRT capture modes and
    refresh rates.

7.  Enable ellipse in driver.


Revision:   Preliminary Production Version 1.1.7
Release Date:  September 20, 1996
=================================================

1.  Added functions to read mode info from ChipsMM.INI for
    Multimedia support.

2.  Fixed a GPF problem when changing color depth dynamically after 
     windowed DOS prompt is created and exited.

3.  Fixed a GPF found when cancelling OSR2 installation.

4.  Fixed a string corruption problem when copy cells in Excel.

5.  Fixed software cursor hang problem in WinBench96 (GWM5).

6.  Fixed Immortal Klowns flashing problem in HiRes or HiColor modes.

7.  Implemented OSR2 refresh rate support.

8.  Fixed refresh rate problem in Mode 3+ when DOS Box --> CRT --> Full
    screen DOS.

9.  Fixed a icon corruption problem after returned from full screen DOS
     prompt.

10. Fixed GPF problems when existing Windows or doing dynamic resolution
     or color depth switching.

11. Fixed garbage during Immortal Klown on 550 STNDD panel machine when
     booted in CRT mode and then do a HotKey switch to panel mode.

Revision:   Preliminary Production Version 1.1.4
Release Date:  August 19, 1996
=================================================

1.    Modified the memory calculations for 800x600 DSTN panels so
      all appropriate modes are available for CRT, LCD, and
      simultaneous display types.

2.    Fixed a cursor corruption problem with the AVI test of
      Windows 95 SCT test.

3.    Fixed a display problem in mode 3+ where pressing <Ctrl-Alt-
      Del> corrupted the display.

4.    Fixed a problem where the Windows 95 logo appeared to flash
      twice when starting up a 6554x machine.

5.    Fixed a problem where the popup menu would corrupt the
      screen on machines using DSTN panels.

6.    Added support for the 5F22 BIOS function for the F65548
      chipset.  The F65545 chipset does not support this function.

7.    Fixed a problem with Direct draw games and Benchmarks having
      low performance.


Revision:   Version 1.1.0
Release Date:  July 11, 1996
============================

1.    Fixed a problem which occurred when the DirectDraw  driver
      was  running with the FoxBear game in the 800x600 and 1024x768
      STNDD panels in simultaneous mode.

2.    Fixed a problem when running the Borland Turbo Debugger.

3.    Fixed a problem where the selected Display Type (LCD, CRT,
      Both) in Full Screen DOS would change when exiting Full Screen
      DOS and returning to the Windows desktop.

4.    Modified the 16BPP modes from 5-5-5(32K color) to 5-6-5(64K
      color).

5.    Fixed a problem with restoring DOS VM in Japanese  Windows
      after changing to the US environment by typing CHEV US command in
      the DOS VM environment.

6.    Fixed the problem with the flashing Windows 95 logo when booting
      Windows 95.

7.    Modified the driver to adjust the video window alignment for
      the high bandwidth modes.

8.    Fixed the problems in VxD.

9.    Fixed the AVI corruption problem with overlay surfaces in
      the 8bpp modes.

10.   Added support for DirectDraw off-screen overlay surfaces for
      software codecs (DVIDEO.DLL).

11.   Adjusted the video display skew for the interlaced modes.

12.   Fixed a problem where panning would not work properly while
      playing an AVI file and switching the display to CRT.

13.   Modified the driver to correct a problem with panning in
      4bpp and 24bpp modes.

14.   Fixed the problem where double screens would appear in the
      4bpp drivers.

15.   Fixed the problem with popup where the popup was
      disappearing when Windows 95 was shutdown and restarted in DOS.

16.   Fixed the problem where the gray text did not appear gray in
      the disabled menu items.

17.   Modified the driver to allow the software cursor to be
      visible in a playback window.

18.   Fixed the cursor problem when running the HCT AVI test.

19.   Fixed a problem with Microsoft's "QuickRes" application.

20.   Fixed the video corruption problem in Merry-Go-Round AVI
      file from Winbench 96.

21.   Fixed the problem in full screen DOS where setting mode 12h
      from mode 3+ sometimes showed a blank screen.

22.   Fixed the problems in the DirectDraw drivers.

23.   Fixed the display corruption problem in mode 72h when
      switching between full screen DOS and the DOS box in Japanese
      Windows 95 by pressing Alt+Enter.

Revision:   Version 1.0.6
Release Date:  June 14, 1996
============================

1.    Fixed a double cursor problem.

2.    Disabled video capture for all 800x600 and 1024x768 DSTN and
      TFT panels in 16bpp modes.

3.    Added CRTPanning=1 in the [Display] section of the SYSTEM.INI
      file to force CRT/NTSC Panning without the BIOS function 5F50
      DL[4] support.

4.    Fixed a problem where the selected Display Type (LCD, CRT, Both)
      in Full Screen DOS would change when exiting Full Screen DOS and
      returning to the Windows desktop.


Revision:   Version 1.0.4
Release Date:  May 21, 1996
============================

1.    Modified the 16BPP modes from 5-5-5(32K color) to 5-6-5(64K
      color).

2.    Fixed the differences in alignment and palette to control
      the noise problem in F65550 ES 1.5/1.6.

3.    Fixed the problem with restoring DOS VM in Japanese Windows
      after changing to the US environment by typing CHEV US command in
      the DOS VM environment.

4.    Fixed the problem with the flashing Windows 95 logo when
      booting Windows 95.

5.    Modified the driver to adjust the video window alignment for
      the high bandwidth modes.

6.    Fixed the problem with Video Capture/Playback and VxD.

7.    Fixed the problems in VxD.

8.    Fixed the AVI corruption problem with overlay surfaces in
      the 8bpp modes.

9.    Added support for DirectDraw off-screen overlay surfaces for
      software codecs (DVIDEO.DLL).

10.   Adjusted the video display skew for the interlaced modes.

11.   Fixed the problem with panning when playing an AVI file &
      switching the display to CRT.

12.   Fixed the problem with the Hardware cursor and Popup while
      loading Windows 95.

13.   Modified the driver to correct a problem with panning in
      4bpp and 24bpp modes.

14.   Fixed the problem where double screens were showing up in
      the 4bpp drivers.

15.   Fixed the problem with Popup where Popup was disappearing
      when Windows 95 was shutdown and restarted in DOS.

16.   Fixed the problem where the gray text was not gray in the
      disabled menu items.

17.   Added panning capability for NTSC/PAL modes.

18.   Disabled vertical interpolation if the MClock is less than
      38MHz for TFT panels.

19.   Disabled vertical interpolation for Flat Panel and
      Simultaneous display modes for STNDD panels.

20.   Enabled the software cursor so that it is now visible in a
      playback window.

21.   Fixed the cursor problem when running the HCT AVI test.

22.   Added a flag to disable error checking when multiple
      multimedia clients want to access the multimedia hardware at the
      same time.

22.   Fixed a problem with Microsoft's "QuickRes" application.

23.   Fixed the video corruption problem in Merry-Go-Round AVI
      file from Winbench 96.

24.   Fixed the problem in full screen MSDOS where setting mode
      12h from mode 3+ sometimes showed a blank screen.

25.   Fixed the problems in the DirectDraw drivers.

27.   Fixed the problem where the display showed garbage in Mode72
      when switching  between the DOS FullScreen and DOS box in
      Japanese Windows 95 by pressing Alt+Enter.


Revision:      Version 1.0.0
Release Date:       March 1, 1996

1. Initial Release.





