Intel(R) PRO/100 LAN+Modem56 CardBus II adapter and
Intel(R) PRO/100 CardBus II LAN-only adapter
June 14, 2000
=======================================================================

Thank you for purchasing the Intel PRO/100 LAN+Modem56 CardBus II 
adapter or Intel PRO/100 CardBus II (LAN-only) adapter. Intel is 
committed to customer satisfaction and timely response to the needs and 
concerns of our customers.

Intel's PRO/100 CardBus II adapters are designed to work with 
portable PC's which include a CardBus PC Card slot. CardBus is the 
next generation PC Card (PCMCIA) standard. It enables portable 
PC's to incorporate a PCI-based 32-bit bus, which improves performance.

The PRO/100 CardBus II adapters incorporate Intel's CardBus Ethernet 
technology and a 56K modem (LAN+Modem56 adapter). It incorporates the 
latest in LAN technology, including advanced power management 
capabilities. It supports ACPI and the CardBus Power Management 
Specification. The modem supports V.90 and K56flex* technology. 

This software release of the PRO/100 CardBus adapter supports Windows 2000,
Windows* 95 OSR2 (950B or higher), Windows 98, and Windows NT* 4.0. A
Windows based LAN diagnostic utility and modem utility are also included. 
Drivers for MS-DOS ODI and NDIS 2 are also provided on the Intel CD. 

If you have compatibility issues not addressed here, or require additional 
information, please refer to your Intel CardBus adapter User's Guide, 
or check our web site for the latest updates.

Remember to register your Intel adapter to receive information about 
future software upgrades and new products.


CONTENTS
========

    1)  Intel PRO/100 CardBus II Adapter Characteristics
    2)  Determining your version Windows 95
    3)  Using the PRO/100 in Windows 95 OSR2 (950B and later)
    4)  Notes on Card Services
    5)  Release Notes/Known Limitations
    6)  CardBus Equipped Portable Computers
    7)  Machine Specific Notes
    8)  Modem Information
    9)  Intel Automated Customer Support


1)  INTEL PRO/100 CardBus II ADAPTER CHARACTERISTICS
    ================================================

    This release of the PRO/100 CardBus II adapters have the following 
    characteristics:
    
    -10/100 Mbps connectivity - Allows portable PCs equipped with a 
      CardBus slot to connect to 100Base-TX Ethernet networks to take 
      advantage of higher network bandwidth. 

    -The PRO/100 adapter takes advantage of the PCI-based 32-bit bus 
     provided by the CardBus slot. This eliminates the bottleneck of a 
     16-bit bus, thus providing high-performance 100 Mbps networking. 
     
    -Auto-negotiation of 10 or 100 Mbps Ethernet connection rate - Upon
     initialization, the adapter will automatically adopt the speed 
     of the network port to which it is attached, allowing it to be 
     used seamlessly on either 10 Mbps (10Base-T) or 100 Mbps 
     (100Base-TX) network segments. 

    -On the LAN+Modem56 adapter, V.90 modem technology allows access to 
     information and e-mail on corporate networks, the Internet, and other
     online services at speeds up to 56Kbps over standard phone lines.
     The V.90 mode enables speeds up to 56Kbps when data is downloaded.
     Upstream data sent from the user travels at the standard V.34 
     rate. The modems at both ends of the call must be V.90 
     compatible to achieve 56K speeds, if not, they will negotiate a 
     standard V.34 connection.

    -Support for using a second PC Card at the same time as the Intel
     CardBus adapter (Type II only) in Windows 95 OSR2 and Windows 98.
    (See machine specific notes for limitations.)

    -Support for using a second PC Card at the same time as the Intel
     CardBus adapter (Type II only) in Windows NT 4.0.

    -Intel software which enhances the ability of Windows 95 OSR2
     (950B) and later to support CardBus multifunction devices.


2)  DETERMINING YOUR VERSION OF WINDOWS 95
    ======================================

    Follow the steps below to determine which version of Windows 95 you 
    are running:

        1  Click on the Start button.
        2  Select Settings.
        3  Select the Control Panel.
        4  Double-click on the System icon. The System Properties dialog 
           box opens.
        5  Select the General tab. Information about your system is 
           displayed, including the version of Windows 95 you are 
           running, under System.

    If 4.00.950 or 4.00.950A is indicated, your version is not supported by 
    the PRO/100 adapter. If 4.00.950B, 4.00.950C or later is reflected, then
    the adapter will work in this environment.  


3)  USING THE PRO/100 LAN+MODEM56 IN WINDOWS 95 OSR2 (950B) and LATER
    =================================================================

    Intel Enhancements for OSR2
    ---------------------------
    Windows 95 version OSR2 (950B) and later support Plug and Play of 
    CardBus devices. However, OSR2 may have problems properly 
    allocating resources to some CardBus multifunction (Ethernet+Modem) 
    devices. The PRO/100 includes software which enhances the ability 
    of Windows 95 OSR2 to support CardBus multifunction devices. 
    This support is implemented in the NDIS4 driver (E100BNT.SYS) and
    E100BCFG.EXE.
    
    E100BCFG.EXE is a configuration program that helps Windows 95 OSR2 
    configure and use the PRO/100 adapter. It is launched after modem 
    installation, following restart. The only indication 
    that it has run will be a dialog box telling the user to restart to
    complete the installation.

    On some machines, the program will detect that particular VxD 
    files from Microsoft may be out of date. If this happens, the 
    user will be informed that it might help to obtain more 
    recent versions of these files. The specific files are:
    CBSS.VXD, PCI.VXD and PCCARD.VXD. Check with your computer
    manufacturer to see if they have any of these updates for your
    computer model. 

        NOTE: DO NOT update these files unless you are experiencing
              problems with the adapter, and you have reviewed the 
              troubleshooting information in the User's Guide. 

    In order to function with Windows 95 OSR2, E100BCFG.EXE places a 
    "forced configuration" onto the slot where the card is inserted.  
    Once this forced configuration is applied, no other card can be 
    inserted into that slot. However, the PRO/100 adapter can still be 
    removed and reinserted into the same slot while the laptop is
    running. The adapter should not be installed into the other slot.

    The forced configuration on the slot can be removed at a later time 
    by running E100BCFG manually (see section on Removing the 
    Forced Configuration below.)

    Removing the Forced Configuration
    ---------------------------------
    The forced configuration on the slot can be removed by running 
    E100BCFG manually. It can be found in the \INTEL\M32AAPPS directory.  
    When double-clicked, the E100BCFG displays a dialog box describing 
    the forced configuration information. Pressing the "Remove 
    Forced Configuration" button will restore the slot to normal.  

    Removing the forced configuration should be done before upgrading to 
    Windows 98.  

    The card must be inserted when E100BCFG is launched.

    Known Limitations in Windows 95 OSR2
    ------------------------------------
    -Under Windows 95 OSR2, once the PRO/100 adapter is installed, no 
     other card can be inserted into the slot where the PRO/100 has been 
     inserted. However, the PRO/100 adapter can be removed and 
     reinserted into the  same slot while the laptop is running. The 
     adapter should not be installed into the other slot, since it would 
     cause a reinstallation of the adapter.

    -Windows 95 may fail to reinitialize the PRO/100 driver when Windows 
     95 comes out of Suspend/Resume.  To make the driver reload in this 
     situation, click on the PC Card (PCMCIA icon) in Control Panel, 
     highlight the adapter and click on Stop. Next, eject the PRO/100 
     adapter and then re-insert it. The PRO/100 adapter will now load.

    -When using Windows 95 OSR2, Toshiba Tecra 500 series 
     laptops require BIOS version 5.7 or later. 

    Upgrading from Windows 95 to Windows 98
    ---------------------------------------
    -If the PRO/100 adapter is installed in Windows 95 OSR2 and you are
     upgrading to Windows 98 the E100BCFG is not needed and the "forced 
     configurations" it creates must be removed. See the section above
     titled "Removing the Forced Configuration" for instructions on how 
     to remove it. 


4)  NOTES ON CARD SERVICES
    ======================

    Windows NT 4.0 and Third Party Card Services
    --------------------------------------------
    -The PRO/100 adapter is not compatible with NT 4.0 Card Services 
     requiring support for PCMCIA proposal 187.

    -SystemSoft CardWizard* 4.1 is now compatible with the 
     CardBus II adapters. 

    -Phoenix CardWare supports the LAN function only. 


5)  RELEASE NOTES/KNOWN LIMITATIONS
    ===============================

    Supported Environments


    ----------------------    

    Driver Name     Description
    
    E100BNT.SYS     NDIS4 Driver for Microsoft Windows 95 (OSR2) and NT 4.0.
    E100BNT5.SYS    NDIS5 Driver for Microsoft Windows 98.
    CBMODEM.SYS     Modem enabler for Windows NT 4.0
    E100BCFG.EXE    PRO/100 configuration program for Windows 95 OSR2
    MDMTESTW.EXE    Windows modem test utility
    E100BODI.COM    DOS 16-bit ODI driver.
    E100B.LAN       DOS 32-bit ODI driver and NetWare* 4.11/5.0 Server driver.
    E100B.DOS       DOS NDIS 2 driver.
    CE100B.LAN      ODI C-Specification driver for NetWare 5.0 Server.


    Known Limitations
    -----------------
    -For Windows 95 OSR2 issues, see section 3 above on Windows 95
  
    -In order to connect to a 100Base-TX Ethernet network, a Category 5
     unshielded twisted pair (UTP) network cable terminating in a male
     RJ-45 connector must be connected to a 100Mbps hub or switch. Check
     with your LAN Administrator if you are not certain of your network
     speed and infrastructure.

    -The PRO/100 adapter is designed to connect to a 100Base-TX network.
     It does not support 100VG-AnyLAN networks.     

    -If you are attempting to use the PRO/100 adapter in a port 
     replicator or docking station, are using Windows 95 and are having 
     problems, there are three alternatives: 

     1. Put the adapter in the notebook rather than the replicator/
        docking station
     2. Manually load the drivers
     3. Use Windows 98 as it appears to support this environment better 
        than Windows 95.

    -When attempting to use the PRO/100 adapter with a 16-bit 
     adapter (e.g. modems, flash cards, ATA cards) in the other slot, it 
     may be necessary to start up with only the PRO/100 installed, then 
     hot-insert the second adapter.

    -On the LAN+Modem adapter, to achieve 56Kbps speed, there can be only one
     digital to analog conversion between the connecting modems.
     Also, the modems at both ends of the call must be .V90 or K56flex
     compatible to achieve 56K speeds, if not, they will negotiate
     a standard V.34 rate. Current FCC regulations limit download
     speeds of the modem to 53Kbps.

    -When running MS-DOS, the PRO/100 CardBus II adapters must be initialized
     by running the CBCOMBO.EXE utility. Usage is as follows:

       CBCOMBO [Optional parameters]

     For the NDIS 2 DOS driver E100B.DOS the CBCOMBO utility must be run from 
     the CONFIG.SYS file during system startup. The usage for this method is as 
     follows:
       DEVICE=\path\CBCOMBO.EXE  [optional parameters]

     NOTE:  For the LAN-only adapter, the NOCOM parameter must be used at all 
     times. Usage:  CBCOMBO NOCOM <Enter>

     NOTE:  A memory exclusion is often required to have the driver properly
     recognize the card. Usage CBCOMBO <Enter>

     Simultaneous dual mode operation of the LAN and Modem functions has limited
     support in the DOS environment. The CardBus II adapter requires that both 
     the LAN and modem function share the same hardware interrupt. Most DOS-
     based LAN and modem communications applications were developed before the 
     PCI bus made interrupt sharing possible and therefore have no support for 
     interrupt sharing. Using the 16-bit ODI driver, specify either NOCOM or 
     NOLAN when loading the CBCOMBO utility (see CB2HELP.HLP for more 
     information about CBCOMBO). The 32-bit ODI driver does not support modems.

     Laptops Running Windows NT 4.0
     ------------------------------
     On newer Toshiba models running Windows NT 4.0 and equipped with the Topic 
     97 controller, the drivers will appear to install correctly. After the 
     first restart, however, the CardBus adapter will not function. To resolve 
     this condition, run TSETUP (the Toshiba setup utility) and change the 
     PC Card mode from Autodetect to 16-bit/Cardbus mode. Repeat the instal-
     lation process.

     Sometimes the default resources selected for NT do not work and the adapter
     will not function. If this happens, you will have to try others. Because of 
     the large number of laptops on the market, it is impossible to track the 
     precise resources for each one. In general, if the default resources don't 
     work, try these first, in the following order:
     
           IRQ:  11, 9, 5, 3
           I/O Memory:  d000, d400, 5b8000.

     When changing these resources, be sure to "cold boot" the laptop (turn it 
     completely off and back on with power switch).


     For other optional parameters, refer to the CB2HELP.HLP file on the 
     Intel CD.


6)  CardBus EQUIPPED PORTABLE COMPUTERS
    ===================================

    The PRO/100 adapter requires a portable computer with a CardBus 
    PC Card Slot. Most laptops introduced after January 1997 incorporate
    CardBus PC Card slots.  If you're not sure if your system supports
    CardBus, contact the manufacturer of your laptop.

    If the adapter fails to fully insert into the slot, it is likely 
    that your computer does not support CardBus. If Windows 95 or 98 
    fails to recognize the PRO/100 adapter when inserted, you may have 
    to get an update from your computer manufacturer. 


7)  MACHINE SPECIFIC NOTES
    ======================

    Visit the Intel web site for updated machine specific information.

    Acer 367D
    ---------
    -The PRO/100 CardBus II adapters are not compatible with this model when 
    running Windows NT 4.0.

    Compaq 7792 with original version of Windows 95 (OSR2) installed by Compaq.
    ---------------------------------------------------------------------------
    The PRO/100 CardBus adapters drivers will not properly install in this 
    model due to Compaq's customization of Windows. The solution is to install a 
    generic version of Windows 95 OSR2 or Windows 98 and then install the 
    PRO/100 adapter.

    Gateway Solo, Model 9100
    ------------------------
    -If you have any problems with this model, try changing the IRQ value.

    Hewlett Packard Omnibook* 800CS
    -------------------------------
    -Requires BIOS version 2.0 or later.  Available from Hewlett 
     Packard web site.

    Micron TransPort Trek
    ---------------------
    -For correct operation under Windows NT, change the resources to IRQ=11 and
    Memory=5B8000.

    Sony 717
    --------
    -The PRO/100 CardBus II adapters are not compatible with this model when 
    running Windows NT 4.0.

    Toshiba Portable Computers 
    --------------------------

    -On newer Toshiba models running Windows NT 4.0 and equipped with the Topic 
     97 controller, the drivers will appear to install correctly. After the 
     first restart, however, the CardBus adapter will not function. To resolve 
     this condition, run TSETUP (the Toshiba setup utility) and change the 
     PC Card mode from Autodetect to 16-bit/Cardbus mode. Repeat the instal-
     lation process.

    -If the driver fails to load in Windows 98, and Device Manager displays a
     yellow exclamation point for the adapter, change the Adaptive Performance
     Tuning setting to the leftmost position. This setting is accessed from
     Intel PROSet, on the Advanced tab.

    -If using Windows 95 OSR2, an operating system patch may be 
     required. Check with Toshiba for more information
    
    -If the PRO/100 adapter does not load in the top PC Card slot
     on Toshiba Tecra* and Portege* computers, there are two remedies:

     1.  Try using the CardBus adapter in the lower slot.
     2.  Disable support for the infrared device by commenting out
         (put a semi-colon ";" in front of) the following lines 
         in the Windows SYSTEM.INI file: 
         ;device=C:\TRANXIT\pumafir.386
    
    -When using Windows 95 OSR2, Toshiba Tecra 500 series 
     laptops require BIOS version 5.7 or later. 

    -Some Toshiba computers require you to run a utility called 
     TSETUP.EXE to put the PCMCIA controller into CardBus mode. 

    -When using the PRO/100 adapter on certain Toshiba computers,
     use of the second PC Card slot is disabled when the computer
     is put into CardBus/16-bit PC Card mode.

     Toshiba Tecra 550
     -----------------
     -Set the IRQ=11 in this model for proper operation in Windows NT 4.

     -The adapter will not function if your Tecra 550 is running the Toshiba 
      version of Windows 95. Upgrade to Windows 98 to solve this issue.


8)  MODEM INFORMATION
    =================

For AT commands and V90 S registers, see the CB2HELP.HLP file on the Intel CD.

New information not included in the help file:

S109 REGISTER
-------------

The firmware contained in this product is designed to initially 
attempt to make a v.90 connection, and then fall back to K56flex if 
the host being dialed does not support v.90. However, the host being
dialed must support v.90 autodetect in order for a v.90 connection
to be initiated by default. At this time many v.90 hosts do not
support autodetect. In such cases it will be necessary to issue an
ATS109=2 command to the modem in order to force a v.90 connection.

Please note that if this command is used and a v.90 connection is
not achieved the modem will fall back directly to v.34. When S109=2,
fall back from v.90 to K56Flex is disabled.  To set this value back
to the default issue an ATS109=1 command. 

In summary, the values of this register and the resultant behavior
are:

S109=1 (default) - Negotiates initially at v.90 if host supports
                   v.90 autodetect. If host does not support 
                   v.90 autodetect or does not support v.90 at
                   all, will negotiate back to K56flex.
S109=2           - Forces v.90 for PCM connects. If host does not
                   support v.90, falls directly back to v.34.

Changing the value of the S109 register can be implemented via the 
following means:

-When using a terminal emulator program, enter ATS109=n (where n is 
 the value desired).
-To implement with Windows 95/98/NT dial up networking, go to
 Control Panel\Modems. Highlight the modem and click Properties.
 Click Connection\Advanced. Enter S109=n (where n is the value
 desired) in the Extra Settings box.


9)  INTEL AUTOMATED CUSTOMER SUPPORT
    ================================

    Get support information and download software updates from Intel's 
    World Wide Web server or from the Intel FTP server.  

    Intel World Wide Web server

    Support:        http://support.intel.com
    Intel News:     news://intelforums.com
    Corporate:      http://www.intel.com
    
    Navigate to a specific product and then look for support information.

    Intel FTP server

    ftp://download.intel.com/support/network/adapter

    Customer Support

    Worldwide access: Intel has technical support centers worldwide. 
    Many of the centers are staffed by technicians who speak the local 
    languages. For a list of all Intel support centers, the telephone 
    numbers, and the times they are open, download document 9089 from 
    one of the automated services.

    If you don't have access to automated services, contact your local 
    dealer or distributor. 

    Before you call...

    You need to be at your computer with your software running and the 
    product documentation at hand.

    The technician may ask for the following:

    *Your address and telephone number
    *The name and model number of the Intel product you are calling 
     about
    *The names and version numbers of the software you are using to 
     operate the Intel product
    *The name and version number of the operating system you are using
    *The computer's manufacturer and model number
    *Expansion boards or add-in cards in your computer
    *The amount of memory in your computer

Customer Support Number:  916-377-7000

Hours:  07:00 - 17:00 Monday through Friday (U.S. Pacific time)


* Third party trademarks and brand names are the property of their owners.
