			INSTALLATION INSTRUCTIONS FOR
	16-BIT NDIS 2.01 DRIVER FOR IBM LAN SERVER DOS REQUESTER WITH
                    THE HP DESKDIRECT LAN ADAPTER (J2973A)

 
 The Network Driver Interface Specification (NDIS) 2.01 is a 16-bit driver
 used by many DOS networking products to gain access to the LAN.
 
 The HP NDIS 2.01 driver is self-configuring, which means the driver will
 automatically locate and read the HP DeskDirect LAN Adapter's
 configuration.  Only the DRIVERNAME parameter needs to be present under
 the [HPFEND] section in the PROTOCOL.INI file.
 
 The HP NDIS 2.01 drivers for IBM LAN Server DOS clients are located on
 this Support Disk:
 
     \IBMLS\DOS\HPFEND.DOS - 16-bit NDIS 2.01 for DOS
 
 IBM LAN Server also requires unique NIF file and OEMSETUP.INF (for IBM LAN
 Server 4.0 DOS Services Program only) located on this Support Disk:
 
     \IBMLS\DOS\OEMSETUP.INF - Installation information file for LAN Server
                               4.0 DOS LAN Services
 
 To install Lan Server 4.0 DOS client with the HP DeskDirect LAN Adapter and
 its NDIS 2.01 driver, follow the procedure under the section labeled "IBM
 LAN Server 4.0 DOS LAN Services Installation" below.
 
 
 IBM LAN Server 4.0 DOS LAN Services Installation
 ================================================
 1.  Install the HP DeskDirect LAN Adapter, and optionally, run HPVGSET.
 
     Follow instructions in the printed manual.
 
 2.  Copy HP NDIS 2.01 driver and an installation file to the hard disk.
 
     Create a directory on the hard disk for the HP driver and installation
     file.  Insert the HP Support Disk into the floppy drive and enter the
     following commands at the DOS prompt:
 
         MKDIR C:\NDIS2
         COPY A:\IBMLS\DOS\HPFEND.DOS C:\NDIS2
         COPY A:\IBMLS\DOS\OEMSETUP.INF C:\NDIS2
 
 3.  Install IBM LAN Server 4.0 DOS Services program.
 
     NOTE: If loading on MS-DOS 6.0 or later with multiple configuration
           blocks, replace the CONFIG.SYS and AUTOEXEC.BAT files with a
           single simple configuration.  After the installation is complete,
           incorporate the changes as another configuration in the original
           multi-configuration CONFIG.SYS and AUTOEXEC.BAT files.
 
     a) Insert "IBM LAN Server DOS LAN Services Disk 1" diskette into the
        floppy disk drive and enter the following commands at the DOS prompt:
 
            A:
            INSTALL
 
     b) When the installation program asks where the OEMSETUP.INF file
        resides, answer with the path name where the HP driver files were
        copied in step 2.  In this example, it should be:
 
            C:\NDIS2
 
     c) Then, follow the instructions on the screen and refer to the IBM
        LAN Server 4.0 DOS Services Installation Guide, when needed, to
        complete the installation procedure.
 
     d) Let the installation program automatically update the CONFIG.SYS
        and AUTOEXEC.BAT files to add the necessary commands to invoke the
        DOS LAN Services program every time the computer is booted.
 
 4.  Reboot the computer.
 
     Reboot the computer to have the changes in the CONFIG.SYS and
     AUTOEXEC.BAT take effect.
 
 The IBM LAN Server 4.0 DOS LAN Services installation is complete.
 
 Note: Please refer to the PROTOCOL.TXT file under \NDIS2 directory of 
       HP Support Disk for more information about "PROTOCOL.INI Parameter
       Definitions".

<End of File>
 
