 =============================================================================
 Build and Installation Notes for Toshiba Windows NT SCI Drivers.
 =============================================================================


 Overview:
 =========

 The Toshiba Windows NT SCI Drivers diskette contains drivers which enable
 the MaxTime and Hardware Setup utilities to run on the Windows NT operating
 system.  To ensure proper installation of these drivers, please follow the
 directions found in this file.

Diskette Contents:
 ==================

 The installation diskette should contain the following files:

    o   MSCOMSTF.DLL        - DLL required by Setup program.
    o   MSCUISTF.DLL        - DLL required by Setup program.
    o   MSDETSTF.DLL        - DLL required by Setup program.
    o   MSINSSTF.DLL        - DLL required by Setup program.
    o   MSSHLSTF.DLL        - DLL required by Setup program.
    o   MSUILSTF.DLL        - DLL required by Setup program.
    o   README.TXT          - This file.
    o   SCI.DL_             - Compressed SCI DLL file.
    o   SCIDRV.SY_          - Compressed SCI Driver file.
    o   SCIVDD.DL_          - Compressed SCI VDD file.
    o   HCI.DL_             - Compressed HCI DLL file.
    o   TPNP.DL_            - Compressed TPNP DLL file.
    o   SETUP.EXE           - Setup and Installation program.
    o   SETUP.INF           - Setup INF file required by Setup program.
    o   MSVCRT20.DL_        - File required by Setup program.
    o   MFC30.DL_           - File required by Setup program.
    o   TOSHREG.RE_         - File containing new registry info.
 

 Setup and Installation:
 =======================

 To properly install the Toshiba Windows NT drivers, place the diskette in
 your floppy drive, go to the "File" menu under Windows NT's File Manager and
 select the "Run..." option.  At the dialog prompt, enter "A:\SETUP.EXE",
 assuming you placed the diskette in drive A.  If you placed the diskette
 in any other drive, you must specify that drive instead of A.  Select the
 "OK" button and follow the directions given by the Setup program.


 Troubleshooting:
 ================
 
 Problem:   Setup fails to install some or all of the driver files:
 
    Cause #1:   Out of disk space.
    Solution:   Free up some disk space and re-run Setup.

    Cause #2:   Can't overwrite previously installed driver file.
    Solution:   Locate the installed driver file on your hard disk
		and rename it.  You will not be able to delete it.  Then
		re-run Setup.

 Problem:    You've installed the drivers, but utilities still do not work.

    Cause #1:   Windows NT has not been properly restarted.
    Solution:   Shutdown Windows NT and restart it. Don't just log out.

    Cause #2:   The drivers were not properly installed.
    Solution:   Try re-installing the drivers and restart Windows NT. If
		problem still persists, contact Toshiba Support.

 Known Limitations & Aberrant Behaviors:
 =======================================

 Some of the Toshiba Windows NT Utilities are 16 bit applications running under
 Windows NT 32 bit operating system.  Because of this fact, Windows NT must
 emulate a 16 bit Windows environment.  It does this through what is called a
 VDM, or "Virtual DOS Machine".  However, Windows NT's emulation is not 100% 
 perfect, and therefore certain idiosyncrasies may occur.  


 Please contact Toshiba Support for any other problems not covered here.
