
TOSHIBA Internal V.90 Modem 

                                                                  1998-12-03

I. Country Selection

 Telecommunication regulations vary from one country to another, so you will 
 need to make sure the internal modem's settings are correct for the country 
 in which it will be used.

  Notes: In some countries, you cannot change the country code.
         Also, this utility is not provided in some countries.

 1) Click Start, point to Programs and TOSHIBA Internal Modem and click
    Country Selection.
 2) Then Country Selection icon will appear on the Windows taskbar.
 3) Left click on the Country Selection icon, the Country Selection List will
    appear.
 4) Select the country in which TOSHIBA Internal V.90 Modem will be used.

 5) Right click on the Country Selection icon, the Menu will appear.

        Setting
                You can change the following settings.

                Flag bitmaps for country selection
                        Set up the flag bitmaps for country selection.
                        The flag bitmaps will show up in the Popup menu.

                AutoRun Mode
                        This option is automatically executed when the OS
                        boots up, and sets the modem to the selected country.

                Open Dail properties dialog box after selection country
                        After selecting the country, the Dialing properties
                        dialog box will open to set the dialing properties.

        Modem Selection
                This dialog will show automatically when the TOSHIBA Internal
                Modem cannot be found. Select COM port number when prompt.

        Dialing Properties
                If you selected this, the Dialing Properties window will
                appear. Please select the country you want.



                                                                     Rev 1.1

