                      INSTALLATION INSTRUCTIONS FOR
           16-BIT NDIS 2.01 DRIVER FOR BANYAN VINES CLIENT WITH
                 THE HP DESKDIRECT LAN ADAPTER (J2973A)


 The NDIS driver HPFEND.DOS in the \NDIS2 directory can be used to configure 
 the HP DeskDirect LAN Adapter as a client in a Banyan Vines network
 environment.
 
 Follow the instructions provided in the README file under \NDIS2 subdirectory 
 of this Support Disk along with the information provided in Banyan Vines 
 documentation.  A sample PROTOCOL.HP is provided in the \VINES directory
 of the HP Support Disk.
 
 During the VINES installation procedure, you will be prompted with the
 following:
 
     PROTOCOL.INI bindings =
     
 enter HPFEND.
 
 Vines is a registered trademark of Banyan, Inc.

<End of File>
