                         EMM386 Trap Problem
 
 This document describes a solution to the EMM386 Trap problem.

 Some computers running MS-DOS EMM386, may trap and halt when PCI drivers
 (or HPVGSET) are loaded.  This is a known incompatibility between EMM386
 and some PCI BIOS implementations.  To prevent this problem, run EMM386
 version 4.49 or later.  Version 4.49 is shipped with MS-DOS 6.22 and is
 also available on this diskette in the \EMM386 directory.

 The \EMM386 directory contains the following files. 
 
     README
     EMM386.EX#
     EMM386.EX^
     MSUPDATE.EXE
     UPDATE.BAT

 To update your version of MS-DOS EMM386, do the following:

   1. Create a temporary directory on the same drive on your PC as the 
      \DOS directory - typically the C: drive.  
    
   2. Change to the temporary directory created in the step above, and
      copy the files in the \EMM386 directory on this diskette.

   3. Run UPDATE.BAT to upgrade the file EMM386.SYS to version 4.49. 
